SECTION 5.5

GIVING INSTRUCTION THAT MAY HAVE TO BE EXECUTED

if00 [pras [$InfoXXYZ-[cs-s|sc-s], $InfoXXYZ-[cs-s|sc-s]]]: instruction

|| ifmt vs ifmt | ifmt vs stream | stream vs ifmt | stream vs stream

|| pras: exists between | qran: not exist between

|| Only for stream(s) and free (not for typed)

|| -- ++ []

if00 [qran [$InfoXXYZ-[cs-s|sc-s], $InfoXXYZ-[cs-s|sc-s]]]: 1^^1

instruction w

instruction x

instruction y

instruction z

1==1

|| SCIL at L1

|| Introductory boundary

|| Terminal boundary

uf00 [qran [$InfoXXYZ-[cs-s|sc-s], $InfoXXYZ-[cs-s|sc-s]]]: 1^^1

instruction w

instruction x

instruction y

instruction z

1==1