SECTION 7.4

POTENTIAL ADDITIONAL INSTRUCTION

if00 [pras [-IfmtXXYZ-[oo-o|xx-o], -IfmtXXYZ-[oo-o|xx-o]]]: instruction

|| pras: exists between | qran: not exist between

|| Only for stream(s) and free (not for typed)

|| -- ++ []

if00 [qran [-IfmtXXYZ-[oo-o|xx-o], -IfmtXXYZ-[oo-o|xx-o]]]: 1^^1

instruction w

instruction x

instruction y

instruction z

1==1

|| SCIL at L1

|| Introductory boundary

|| Terminal boundary

af00 [qran [-IfmtXXYZ-[oo-o|xx-o], -IfmtXXYZ-[oo-o|xx-o]]]: 1^^1

instruction w

instruction x

instruction y

instruction z

1==1

uf00: 1^^1

instruction w

instruction x

instruction y

instruction z

1==1