**SECTION 5.6**

**GIVING INSTRUCTION THAT HAS SIBLING**

ftry [pras [$IfmtXXYZ-[cs-s|sc-s], $IfmtXXYZ-[cs-s|sc-s]]]: instruction

atry [qran [$IfmtXXYZ-[cs-s|sc-s], $IfmtXXYZ-[cs-s|sc-s]]]: instruction

then: instruction