SECTION 5.6

GIVING INSTRUCTION THAT HAS SIBLING

ip00 [pras [$IfmtXXYZ-[cs-s|sc-s], $IfmtXXYZ-[cs-s|sc-s]]]: instruction

op00 [qran [$IfmtXXYZ-[cs-s|sc-s], $IfmtXXYZ-[cs-s|sc-s]]]: instruction

up00: instruction