SECTION 5.6

GIVING INSTRUCTION THAT HAS SIBLING

ip00 [pras [$IfmtXXYZ-[ox-x|xo-x], $IfmtXXYZ-[ox-x|xo-x]]]: instruction

op00 [qran [$IfmtXXYZ-[ox-x|xo-x], $IfmtXXYZ-[ox-x|xo-x]]]: instruction

up00: instruction