SECTION 5.6

GIVING INSTRUCTION THAT HAS ALTERNATIVE (SIBLING)

ip00 [pras [-IfmtXXYZ-[ox-x|xo-x], -IfmtXXYZ-[ox-x|xo-x]]]: instruction

op00 [qran [-IfmtXXYZ-[ox-x|xo-x], -IfmtXXYZ-[ox-x|xo-x]]]: instruction

up00: instruction